{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["设备参数","性能特点"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"设备参数","index":0,"n_rows":18,"n_cols":3,"rows_kept":18,"merged":[[0,0,0,2],[1,0,1,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2]],"flags":["formulas_cached_only"]}
["电解质分析仪设备技术参数"]
["测量指标"]
["项目","测量范围","测量精度"]
["K","0.50-15.00mmol/L","CV≤1.0%"]
["Na","30.0-200.0mmol/L","CV≤1.0%"]
["CL","30.0-200.0mmol/L","CV≤1.0%"]
["TCO2","5.0-60.0mmol/L","CV≤4.0%"]
[]
["规格参数"]
["项目","内容"]
["标本形式","血浆、血清、全血或其它组织体液"]
["测量时间","≤30S（从吸样到显示测量数据）"]
["标本量","≥75ul"]
["数据输出","LCD触摸液晶显示器、内置打印机"]
["接口","RS232"]
["电源","AC220V±22V,50HZ±1HZ，120VA"]
["工作环境","温度5-40℃,湿度≤80%"]
["重量","主机≤11kg\n选配自动采样器≤5 kg\n"]

{"sheet":"性能特点","index":1,"n_rows":16,"n_cols":2,"rows_kept":16,"merged":[[0,0,0,1]],"flags":["formulas_cached_only"]}
["性能特点"]
[1,"全程计算机监控，确保高精度和稳定性"]
[2,"大屏幕高清触摸屏"]
[3,"24小时全自动运行检测"]
[4,"电极诊断功能，电极异常提示功能，电极活化预示功能"]
[5,"优化的液路设计"]
[6,"自动气泡检测"]
[7,"机内自检功能"]
[8,"安全环保的全封闭试剂包"]
[9,"试剂量自动统计功能"]
[10,"断电数据自动保持功能"]
[11,"完善的数据贮存、传输、查询、打印功能"]
[12,"质控校正程序"]
[13,"打印31天质控图"]
[14,"39位自动采样器（选购件），急诊样品即插即测"]
[15,"高品质免维护ISE电极"]